%!TEX TS-program = pdflatexmk
%!TEX root = test.tex

% Copyright (c) 2018 - 2021, Martin Scheidt (ISC license)
% Permission to use, copy, modify, and/or distribute this file for any purpose with or without fee is hereby granted, provided that the above copyright notice and this permission notice appear in all copies.

\node[blue] at (4,0) {\large test messure symbols};

\foreach \i in {1,2,3}{% base coordinate
  \coordinate (A\i) at ($(0,0) + 2*(0,-\i)$);% base coordinate
  \coordinate (B\i) at ($(8,0) + 2*(0,-\i)$);% base coordinate
}

\foreach \i in {1,2}{% draw main tracks on base coordinate
  \maintrack (A\i) --   (B\i);
}

\foreach \i in {1,2}{% coordinates for testing symbols
  \coordinate (X\i-1) at ($(1,0) + 2*(0,-\i)$);
  \coordinate (X\i-2) at ($(3,0) + 2*(0,-\i)$);
  \coordinate (X\i-3) at ($(5,0) + 2*(0,-\i)$);
  \coordinate (X\i-4) at ($(7,0) + 2*(0,-\i)$);
}

\trackdistance between (3,-1) and (X1-2) label (4,50);
\trackdistance between (X1-2) and (X2-3) label (\SI[math-rm=\mathsf]{6,50}{\metre});
\trackdistance between (X1-4) and (X2-4) label (5,50);

\tikzset{hectometer base={(A3)},orientation=right};
\hectometer[] at (X2-1) mileage (\SI[math-rm=\mathsf]{6,505}{\kilo\metre});
\hectometer[shift label={(0.3,-1)}] at (X2-2) mileage (name);
% \measureline between (a) and (b);